Determination of oxygen ingress and carbon dioxide loss through plastic bottles using permeation simulation with hydrogen
J. Schneider, M. Orzinski, W. Hunger, BrewingScience  60 (2007) 55–59.