Estimation of Natural Ventilation Rates in an Office Room with 145 mm-Diameter Circular Openings Using the Occupant-Generated Tracer-Gas Method
H. Seol, D. Arztmann, N. Kim, A. Balderrama, Sustainability 15 (2023).

Design Framework for Multiple Infeed DC-Microgrids in Industrial Applications
D. Schaab, P. Spanier, M. Ehlich , E. Fosselmann, eds., Design Framework for Multiple Infeed DC-Microgrids in Industrial Applications, IEEE, Piscataway, NJ, 2022.

Load shifting potential of electric vehicles using management systems for increasing renewable energy share in smart grids
M. Schaffer, F.C. Bollhöfer, J. Üpping, International Journal of Energy Production and Management 7 (2022) 101–113.