Compression properties of glued laminated timber and tensile properties of gluelam lamellas from oil palm wood
K. Frühwald-König, L. Heister, Wood Material Science and Engineering 19 (2024) 1101–1116.

Dewatering behavior of wet oil palm sawn timber during flat compression
N. Kölli, Wood Material Science &; Engineering (2024) 1–15.

Compression Density as an Alternative to Identify an Optimal Moisture Content for High Shear Wet Granulation as an Initial Step for Spheronisation.
S. Ramm, R. Fulek, V.A. Eberle, C. Kiera, U. Odefey, M. Pein-Hackelbusch, Pharmaceutics 14 (2022).