Estimation of Natural Ventilation Rates in an Office Room with 145 mm-Diameter Circular Openings Using the Occupant-Generated Tracer-Gas Method
H. Seol, D. Arztmann, N. Kim, A. Balderrama, Sustainability 15 (2023).