Operation of anaerobic filter compared with an anaerobic moving bed bioreactor for the treatment of waste water from hydrothermal carbonization of fine mulch
J.F. Meier, U. Austermann-Haun, J. Fettig, H. Liebe, M. Wichern, Water Science &; Technology 76 (2017) 2065–2074.